## Addendum 1 “PATROL RIFLES”

Montgomery County Government Purchasing Department

Phone: (93 I) 648 - 5720

Fax: (931)553-5151

P.O. Box 368

Clarksville, TN

37041-0368

On “Delivery, bottom of cover page in original invitation to bid: is changed from ten days from order to 5 weeks as stated below:

IN COMPLIANCE WITH THE ABOVE INVITATION FOR BIDS, AND SUBJECT TO ALL THE CONDITIONS THEREOF, THE UNDERSIGNED OFFERS, AND AGREES, IF THIS BID BE ACCEPTED WITHIN, 30 DAYS FROM THE DATE OF THE OPENING, TO FURNISH ANY OR ALL OF THE ITEMS UPON WHICH PRICES ARE QUOTED, AT THE PRICE SET OPPOSITE EACH ITEM AND, UNLESS OTHERWISE SPECIFIED WITHIN, **5 (Five) WEEKS AFTER OF ORDER**.

In item 5 “USE OF TRADE NAME”: The Sheriff’s Office is seeking fully assembled, “Turn Key” Patrol Rifles. Description of items listed must meet or exceed the specifications listed in Original Invitation to Bid and applies to all components listed on the original bid. For example, the “PMAG 30 AR/M4, Gen M3 Window” Part Number MAG556, manufactured by Magpul does meet or exceed the specifications of the “Troy Battle Magazine”.

If bidding on other than the make, model, or brand specified or such detailed descriptive specifications, the manufacturer's name and catalogue reference, together with specifications therefore must be given or other information given **(CLEARLY STATED ON THE BID SHEET IN EVERY INSTANCE)** to enable the Purchasing Agent to determine the suitability, or otherwise. We will review alternatives at bid opening.

The rifle itself should adhere to the following detailed specifications and criteria for response, repair, and replacement as detailed below. This an expanded specification for the build and delivery of a complete, bore sighted, street ready patrol rifle with following services:

-14.5 inch pinned and welded barrel length to include 4150 chrome moly steel and corrosion resistant barrel (CrMoV) steel with a nitride finish. (40.64cm length). Barrel twist on the 14.5-inch barrel of 1/8, right hand, with “Troy” TPRS Muzzle Break suppressor ready flash hider. Troy’s quick detach suppressor is the approved and implemented suppressor for our agency.

-12.5” SOCC Gen 2 Series, low profile M-Lok textured rail and squid grips.

**- “**Troy” Tritium Battle Sight, standard folding, flip up sights**.**

# - “B5 Systems” BRAVO Mil-Spec Stock, polymer and collapsible

- Pneuma Gas Diverting Ambi Charging Handle, ambidextrous design, gas defusing channels with large latches and texture on the latches for a nonslip surface.

- Ergo Grip “TROY” 3″ SOCC-VFG, low profile, one piece, vertical grip. Machined from billet T6 aluminum, Weighing in at no more than 2.8 oz. compatible to any M-LOK rail with the included mounting hardware. U.S. Military Specification Type III black hard coat anodized.

- Bolt Carrier Group, Full-mass, M16-profile 8620 alloy carrier with Carpenter 158 bolt machined from bar stock that is properly Magnetic Particle Inspected (MP), Marked "MPI", 4140 billet extractor, heat-treated, shot-peened, Manganese-Phosphate coating, properly staked carrier key and Billet 4140 gas key, seated with staked Grade-8 fasteners, with chrome lining, finish through the carrier, gas key, and bolt -head.

- Disconnector, precision ground, S7 Tool Steel, EDM wire cut with gas phased nitride finish

- Upper and lower receiver with flared magazine well, aircraft grade 7075

- 2-piece “Troy” buffer, high reliability, recoil dampening stainless steel with gas phased nitride finish

- Hammer and trigger, mil spec, with nickel Teflon coating

- Troy T-sling- Padded Black, Bio Thane adjustment handle with two stainless steel quick detach, center button releases

- Fire Selector switch, ambidextrous with one short leg, one long leg and reversible.

- Folding sights and optics will be bore sighted via bore mounted laser device. Folding sights and optics will be co-witnessed prior to delivery.

- Bolt, Bolt Carrier, extractor, receiver, and barrel must have matching serial numbers and as components are replaced the same serial number will be used with an “A” identifier, then “B” identifier etc.

- Same day response during normal business hours for repair or replacement and 24 hour response for emergency or exigent circumstances.

- Automatic backfill and loan of any rifle that is taken out of service for any investigative purposes.

- Lifetime warranty on rifle excluding normal wear and tear of chamber throat, barrel, gas system or other parts subject to industry standard acceptable degradation.

In item 7 “IMPORTANT - To be acceptable” Electronic delivery of Bid response is acceptable by the time line listed in the original invitation to bid as noted at the bottom of this paragraph.

Any future request for information concerning this Bid should be forwarded via email to [elblack@mcgtn.net](mailto:elblack@mcgtn.net). The deadline for any future questions, concerns, or clarifications is 4:30pm CST on March 20, 2024. The final addendum, if necessary, will be emailed to all invitees no later than March 21, 2024, 4:30pm CST.